PCBNEW-BOARD Version 1 date Thu 25 Aug 2011 11:29:56 PM CEST

# Created by Pcbnew(2011-07-16 BZR 3051)-testing

$GENERAL
encoding utf-8
LayerCount 2
Ly 1FFF8001
EnabledLayers 1FFF8001
Links 6
NoConn 1
Di 21848 21790 35306 32505
Ndraw 0
Ntrack 14
Nzone 0
BoardThickness 630
Nmodule 4
Nnets 4
$EndGENERAL

$SHEETDESCR
Sheet A4 11700 8267
Title ""
Date "25 aug 2011"
Rev ""
Comp ""
Comment1 ""
Comment2 ""
Comment3 ""
Comment4 ""
$EndSHEETDESCR

$SETUP
InternalUnit 0.000100 INCH
Layers 2
Layer[0] Back signal
Layer[15] Front signal
TrackWidth 80
TrackClearence 100
ZoneClearence 200
TrackMinWidth 80
DrawSegmWidth 150
EdgeSegmWidth 150
ViaSize 350
ViaDrill 250
ViaMinSize 350
ViaMinDrill 200
MicroViaSize 200
MicroViaDrill 50
MicroViasAllowed 0
MicroViaMinSize 200
MicroViaMinDrill 50
TextPcbWidth 120
TextPcbSize 600 800
EdgeModWidth 150
TextModSize 600 600
TextModWidth 120
PadSize 600 600
PadDrill 0
Pad2MaskClearance 100
AuxiliaryAxisOrg 0 0
PcbPlotParams (pcbplotparams (layerselection 3178497) (usegerberextensions true) (excludeedgelayer true) (linewidth 60) (plotframeref false) (viasonmask false) (mode 1) (useauxorigin false) (hpglpennumber 1) (hpglpenspeed 20) (hpglpendiameter 15) (hpglpenoverlay 2) (pscolor true) (psnegative false) (psa4output false) (plotreference true) (plotvalue true) (plotothertext true) (plotinvisibletext false) (padsonsilk false) (subtractmaskfromsilk false) (outputformat 1) (mirror false) (drillshape 1) (scaleselection 1) (outputdirectory ""))
$EndSETUP

$EQUIPOT
Na 0 ""
St ~
$EndEQUIPOT
$EQUIPOT
Na 1 "GND"
St ~
$EndEQUIPOT
$EQUIPOT
Na 2 "N-000002"
St ~
$EndEQUIPOT
$EQUIPOT
Na 3 "N-000003"
St ~
$EndEQUIPOT
$NCLASS
Name "Default"
Desc "This is the default net class."
Clearance 100
TrackWidth 80
ViaDia 350
ViaDrill 250
uViaDia 200
uViaDrill 50
AddNet ""
AddNet "GND"
AddNet "N-000002"
AddNet "N-000003"
$EndNCLASS
$MODULE R3
Po 22469 24996 2700 15 00200000 4E56BB00 ~~
Li R3
Cd Resitance 3 pas
Kw R
Sc 4E56BB00
AR /4E56BA66
Op 0 A 0
T0 0 0 550 500 2700 80 N V 21 N "R1"
T1 0 0 550 500 2700 80 N I 21 N "R"
DS -1500 0 -1300 0 120 21
DS 1500 0 1300 0 120 21
DS 1300 0 1300 -400 120 21
DS 1300 -400 -1300 -400 120 21
DS -1300 -400 -1300 400 120 21
DS -1300 400 1300 400 120 21
DS 1300 400 1300 0 120 21
DS -1300 -200 -1100 -400 120 21
$PAD
Sh "1" C 550 550 0 0 2700
Dr 320 0 0
At STD N 00E0FFFF
Ne 3 "N-000003"
Po -1500 0
$EndPAD
$PAD
Sh "2" C 550 550 0 0 2700
Dr 320 0 0
At STD N 00E0FFFF
Ne 1 "GND"
Po 1500 0
$EndPAD
$SHAPE3D
Na "discret/resistor.wrl"
Sc 0.300000 0.300000 0.300000
Of 0.000000 0.000000 0.000000
Ro 0.000000 0.000000 0.000000
$EndSHAPE3D
$EndMODULE  R3
$MODULE R3
Po 34685 30626 900 15 00200000 4E56BB02 ~~
Li R3
Cd Resitance 3 pas
Kw R
Sc 4E56BB02
AR /4E56BA6D
Op 0 A 0
T0 0 0 550 500 900 80 N V 21 N "R3"
T1 0 0 550 500 900 80 N I 21 N "R"
DS -1500 0 -1300 0 120 21
DS 1500 0 1300 0 120 21
DS 1300 0 1300 -400 120 21
DS 1300 -400 -1300 -400 120 21
DS -1300 -400 -1300 400 120 21
DS -1300 400 1300 400 120 21
DS 1300 400 1300 0 120 21
DS -1300 -200 -1100 -400 120 21
$PAD
Sh "1" C 550 550 0 0 900
Dr 320 0 0
At STD N 00E0FFFF
Ne 1 "GND"
Po -1500 0
$EndPAD
$PAD
Sh "2" C 550 550 0 0 900
Dr 320 0 0
At STD N 00E0FFFF
Ne 2 "N-000002"
Po 1500 0
$EndPAD
$SHAPE3D
Na "discret/resistor.wrl"
Sc 0.300000 0.300000 0.300000
Of 0.000000 0.000000 0.000000
Ro 0.000000 0.000000 0.000000
$EndSHAPE3D
$EndMODULE  R3
$MODULE R3
Po 26803 30630 900 15 00200000 4E56BB04 ~~
Li R3
Cd Resitance 3 pas
Kw R
Sc 4E56BB04
AR /4E56BA7E
Op 0 A 0
T0 0 0 550 500 900 80 N V 21 N "R4"
T1 0 0 550 500 900 80 N I 21 N "R"
DS -1500 0 -1300 0 120 21
DS 1500 0 1300 0 120 21
DS 1300 0 1300 -400 120 21
DS 1300 -400 -1300 -400 120 21
DS -1300 -400 -1300 400 120 21
DS -1300 400 1300 400 120 21
DS 1300 400 1300 0 120 21
DS -1300 -200 -1100 -400 120 21
$PAD
Sh "1" C 550 550 0 0 900
Dr 320 0 0
At STD N 00E0FFFF
Ne 1 "GND"
Po -1500 0
$EndPAD
$PAD
Sh "2" C 550 550 0 0 900
Dr 320 0 0
At STD N 00E0FFFF
Ne 3 "N-000003"
Po 1500 0
$EndPAD
$SHAPE3D
Na "discret/resistor.wrl"
Sc 0.300000 0.300000 0.300000
Of 0.000000 0.000000 0.000000
Ro 0.000000 0.000000 0.000000
$EndSHAPE3D
$EndMODULE  R3
$MODULE test_connected_pins
Po 29299 25000 0 15 4E56BE73 4E56BAFF ~~
Li test_connected_pins
Sc 4E56BAFF
AR /4E56BA63
Op 0 0 0
T0 0 3500 600 600 0 120 N V 21 N "R2"
T1 0 -2750 600 600 0 120 N V 21 N "R"
DS -1000 250 -250 250 150 21
DS -250 1250 750 1250 150 21
DS 250 500 250 1250 150 21
DS 500 -1250 500 250 150 21
DS 500 250 -250 750 150 21
DS 2000 -1250 500 -1250 150 21
DS -2250 -1250 -1000 -1250 150 21
DS -1000 -1250 -1000 2000 150 21
DS -1000 2000 -2250 2000 150 21
DS -2750 -1750 2500 -1750 150 21
DS 2500 -1750 2500 2500 150 21
DS 2500 2500 -2750 2500 150 21
DS -2750 2500 -2750 -1750 150 21
$PAD
Sh "1" R 600 600 0 0 0
Dr 0 0 0
At SMD N 00888000
Ne 3 "N-000003"
Po -2500 -1500
$EndPAD
$PAD
Sh "2" R 600 600 0 0 0
Dr 0 0 0
At SMD N 00888000
Ne 2 "N-000002"
Po 2250 -1500
$EndPAD
$PAD
Sh "1" R 600 600 0 0 0
Dr 0 0 0
At SMD N 00888000
Ne 3 "N-000003"
Po -2500 2250
$EndPAD
$EndMODULE  test_connected_pins
$TRACK
Po 0 26803 32130 34681 32130 80 -1
De 15 0 1 0 C00000
Po 0 34681 32130 34685 32126 80 -1
De 15 0 1 0 C00000
Po 0 22469 26496 22469 30213 80 -1
De 15 0 1 0 400000
Po 0 24386 32130 26803 32130 80 -1
De 15 0 1 0 800000
Po 0 22469 30213 24386 32130 80 -1
De 15 0 1 0 0
Po 0 26803 32130 31507 32130 80 -1
De 15 0 1 0 400000
Po 0 31507 32130 31531 32106 80 -1
De 15 0 1 0 0
Po 0 31549 23500 33709 23500 80 -1
De 15 0 2 0 400000
Po 0 34685 24476 34685 29126 80 -1
De 15 0 2 0 800000
Po 0 33709 23500 34685 24476 80 -1
De 15 0 2 0 0
Po 0 26799 27250 26799 29126 80 -1
De 15 0 3 0 400000
Po 0 26799 29126 26803 29130 80 -1
De 15 0 3 0 800000
Po 0 22469 23496 26795 23496 80 -1
De 15 0 3 0 400000
Po 0 26795 23496 26799 23500 80 -1
De 15 0 3 0 800000
$EndTRACK
$ZONE
$EndZONE
$EndBOARD
